
18-pin Flash/EEPROM 8-Bit Microcontrollers

• PIC16F83
• PIC16F84
• PIC16CR83
• PIC16CR84
• Extended voltage range devices available
  (PIC16LF8X, PIC16LCR8X)


High Performance RISC CPU Features:

• Only 35 single word instructions to learn
• All instructions single cycle except for program
  branches which are two-cycle
• Operating speed: DC - 10 MHz clock input
  DC - 400 ns instruction cycle
• 14-bit wide instructions
• 8-bit wide data path
• 15 special function hardware registers
• Eight-level deep hardware stack
• Direct, indirect and relative addressing modes
• Four interrupt sources:
  - External RB0/INT pin
  - TMR0 timer overflow
  - PORTB<7:4> interrupt on change
  - Data EEPROM write complete
• 1000 erase/write cycles Flash program memory
• 10,000,000 erase/write cycles EEPROM data memory
• EEPROM Data Retention > 40 years

Peripheral Features:

• 13 I/O pins with individual direction control
• High current sink/source for direct LED drive
- 25 mA sink max. per pin
- 20 mA source max. per pin
• TMR0: 8-bit timer/counter with 8-bit
  programmable prescaler

Special Microcontroller Features:

• In-Circuit Serial Programming (ICSP™) - via two
  pins (ROM devices support only Data EEPROM
  programming)
• Power-on Reset (POR)
• Power-up Timer (PWRT)
• Oscillator Start-up Timer (OST)
• Watchdog Timer (WDT) with its own on-chip RC
  oscillator for reliable operation
• Code-protection
• Power saving SLEEP mode
• Selectable oscillator options

CMOS Flash/EEPROM Technology:

• Low-power, high-speed technology
• Fully static design
• Wide operating voltage range:
  - Commercial: 2.0V to 6.0V
  - Industrial: 2.0V to 6.0V
• Low power consumption:
  - < 2 mA typical @ 5V, 4 MHz
  - 15 mA typical @ 2V, 32 kHz
  - < 1 mA typical standby current @ 2v
