ATtiny13

8-bit AVR with 1K Bytes In-System Programmable Flash

• High Performance, Low Power AVR® 8-Bit Microcontroller
• Advanced RISC Architecture
  – 120 Powerful Instructions – Most Single Clock Cycle Execution
  – 32 x 8 General Purpose Working Registers
  – Fully Static Operation
  – Up to 20 MIPS Througput at 20 MHz
• Non-volatile Program and Data Memories
  – 1K Byte of In-System Programmable Program Memory Flash
    Endurance: 10,000 Write/Erase Cycles
  – 64 Bytes In-System Programmable EEPROM
    Endurance: 100,000 Write/Erase Cycles
  – 64 Bytes Internal SRAM
  – Programming Lock for Self-Programming Flash Program 
    and EEPROM Data Security
• Peripheral Features
  – One 8-bit Timer/Counter with Prescaler and Two PWM Channels
  – 4-channel, 10-bit ADC with Internal Voltage Reference
  – Programmable Watchdog Timer with Separate On-chip Oscillator
  – On-chip Analog Comparator
• Special Microcontroller Features
  – debugWIRE On-chip Debug System
  – In-System Programmable via SPI Port
  – External and Internal Interrupt Sources
  – Low Power Idle, ADC Noise Reduction, and Power-down Modes
  – Enhanced Power-on Reset Circuit
  – Programmable Brown-out Detection Circuit
  – Internal Calibrated Oscillator
• I/O and Packages
  – 8-pin PDIP/SOIC: Six Programmable I/O Lines
  – 20-pad MLF: Six Programmable I/O Lines
• Operating Voltage:
  – 1.8 - 5.5V for ATtiny13V
  – 2.7 - 5.5V for ATtiny13
• Speed Grade
  – ATtiny13V: 0 - 4 MHz @ 1.8 - 5.5V, 0 - 10 MHz @ 2.7 - 5.5V
  – ATtiny13: 0 - 10 MHz @ 2.7 - 5.5V, 0 - 20 MHz @ 4.5 - 5.5V
• Industrial Temperature Range
• Low Power Consumption
  – Active Mode:    1 MHz, 1.8V: 240µA
  – Power-down Mode:    < 0.1µA at 1.8V