Protel Design System Design Rule Check
PCB File : PCB2.PCB
Date     : 27-Oct-2003
Time     : 21:23:28

Processing Rule : Clearance Constraint (Gap=14mil) (On the board ),(On the board )
Rule Violations :0

Processing Rule : Width Constraint (Min=28mil) (Max=28mil) (Prefered=28mil) (On the board )
Rule Violations :0

Processing Rule : Short-Circuit Constraint (Allowed=Not Allowed) (On the board ),(On the board )
Rule Violations :0

Processing Rule : Broken-Net Constraint ( (On the board ) )
Rule Violations :0

Processing Rule : Short-Circuit Constraint (Allowed=Not Allowed) (On the board ),(On the board )
Rule Violations :0

Processing Rule : Broken-Net Constraint ( (On the board ) )
Rule Violations :0


Violations Detected : 0
Time Elapsed        : 00:00:00