
8-Bit CMOS Microcontrollers with A/D Converter

• PIC16C710
• PIC16C71
• PIC16C711
• PIC16C715

PIC16C71X Microcontroller Core Features:

• High-performance RISC CPU
• Only 35 single word instructions to learn
• All single cycle instructions except for program
  branches which are two cycle
• Operating speed: DC - 20 MHz clock input
DC - 200 ns instruction cycle
• Up to 2K x 14 words of Program Memory,
  up to 128 x 8 bytes of Data Memory (RAM)
• Interrupt capability
• Eight level deep hardware stack
• Direct, indirect, and relative addressing modes
• Power-on Reset (POR)
• Power-up Timer (PWRT) and
  Oscillator Start-up Timer (OST)
• Watchdog Timer (WDT) with its own on-chip RC
  oscillator for reliable operation
• Programmable code-protection
• Power saving SLEEP mode
• Selectable oscillator options
• Low-power, high-speed CMOS EPROM
  technology
• Fully static design
• Wide operating voltage range: 2.5V to 6.0V
• High Sink/Source Current 25/25 mA
• Commercial, Industrial and Extended temperature
  ranges
• Program Memory Parity Error Checking Circuitry
  with Parity Error Reset (PER) (PIC16C715)
• Low-power consumption:
  - < 2 mA @ 5V, 4 MHz
  - 15mA typical @ 3V, 32 kHz
  - < 1mA typical standby current

PIC16C71X Peripheral Features:

• Timer0: 8-bit timer/counter with 8-bit prescaler
• 8-bit multichannel analog-to-digital converter
• Brown-out detection circuitry for
  Brown-out Reset (BOR)
• 13 I/O Pins with Individual Direction Control