
PIC16F716

8-bit Flash-based Microcontroller with A/D Controller
Enhanced Capture/Compare PWM

Microcontroller Core Features:

• High-performance RISC CPU
• Only 35 single-word instructions to learn
 - All single-cycle instructions except for
  program branches which are two-cycle
• Operating speed: DC - 20 MHz clock input
  DC - 200 ns instruction cycle
• Interrupt capability
  (up to 7 internal/external interrupt sources)
• 8-level deep hardware stack
• Direct, Indirect and Relative Addressing modes
  
Special Microcontroller Features

• Power-on Reset (POR)
• Power-up Timer (PWRT) and
  Oscillator Start-up Timer (OST)
• Watchdog Timer (WDT) with its own on-chip RC
  oscillator for reliable operation
• Dual level Brown-out Reset circuitry
  - 2.5 VBOR (Typical)
  - 4.0 VBOR (Typical)
• Programmable code protection
• Power saving Sleep mode
• Selectable oscillator options
• Fully static design
• In-Circuit Serial Programming? (ICSP™)
  CMOS Technology
• Wide operating voltage range:
  - Industrial: 2.0V to 5.5V
  - Extended: 3.0V to 5.5V
• High Sink/Source Current 25/25 mA
• Wide temperature range:
  - Industrial: -40°C to 85°C
  - Extended: -40°C to 125°C

 Low-Power Features:

• Standby Current:
  - 100 nA @ 2.0V, typical
• Operating Current:
  - 14µA @ 32 kHz, 2.0V, typical
  - 120µA @ 1 MHz, 2.0V, typical
• Watchdog Timer Circuit:
  - 1µA @ 2.0V, typical
• Timer1 Oscillator Current:
  - 3.0µA @ 32 kHz, 2.0V, typical

Peripheral Features:

• Timer0: 8-bit timer/counter with 8-bit prescaler
• Timer1: 16-bit timer/counter with prescaler
  can be incremented during Sleep via external
  crystal/clock
• Timer2: 8-bit timer/counter with 8-bit period
  register, prescaler and postscaler
• Enhanced Capture, Compare, PWM module:
  - Capture is 16-bit, max. resolution is 12.5 ns
  - Compare is 16-bit, max. resolution is 200 ns
  - PWM maximum resolution is 10-bit
  - Enhanced PWM:
  - Single, Half-Bridge and Full-Bridge modes
  - Digitally programmable dead-band delay
  - Auto-shutdown/restart
• 8-bit multi-channel Analog-to-Digital converter
• 13 I/O pins with individual direction control
• Programmable weak pull-ups on PORTB
