
• PIC16F73
• PIC16F74
• PIC16F76
• PIC16F77

28/40-Pin 8-Bit CMOS FLASH Microcontrollers

High Performance RISC CPU:

• High performance RISC CPU
• Only 35 single word instructions to learn
• All single cycle instructions except for program
  branches which are two-cycle
• Operating speed: DC - 20 MHz clock input
  DC - 200 ns instruction cycle
• Up to 8K x 14 words of FLASH Program Memory,
  Up to 368 x 8 bytes of Data Memory (RAM)
• Pinout compatible to the PIC16C73B/74B/76/77
• Pinout compatible to the PIC16F873/874/876/877
• Interrupt capability (up to 12 sources)
• Eight level deep hardware stack
• Direct, Indirect and Relative Addressing modes
• Processor read access to program memory

Special Microcontroller Features:

• Power-on Reset (POR)
• Power-up Timer (PWRT) and
  Oscillator Start-up Timer (OST)
• Watchdog Timer (WDT) with its own on-chip RC
  oscillator for reliable operation
• Programmable code protection
• Power saving SLEEP mode
• Selectable oscillator options
• In-Circuit Serial Programming? (ICSP?) via two
  pins

Peripheral Features:

• Timer0: 8-bit timer/counter with 8-bit prescaler
• Timer1: 16-bit timer/counter with prescaler,
  can be incremented during SLEEP via external
  crystal/clock
• Timer2: 8-bit timer/counter with 8-bit period
  register, prescaler and postscaler
• Two Capture, Compare, PWM modules
  - Capture is 16-bit, max. resolution is 12.5 ns
  - Compare is 16-bit, max. resolution is 200 ns
  - PWM max. resolution is 10-bit
• 8-bit, up to 8-channel Analog-to-Digital converter
• Synchronous Serial Port (SSP) with SPI (Master
  mode) and I2C (Slave)
• Universal Synchronous Asynchronous Receiver
  Transmitter (USART/SCI)
• Parallel Slave Port (PSP), 8-bits wide with
  external RD, WR and CS controls (40/44-pin only)
• Brown-out detection circuitry for
  Brown-out Reset (BOR)

CMOS Technology:

• Low power, high speed CMOS FLASH technology
• Fully static design
• Wide operating voltage range: 2.0V to 5.5V
• High Sink/Source Current: 25 mA
• Industrial temperature range
• Low power consumption:
  - < 2 mA typical @ 5V, 4 MHz
  - 20 µA typical @ 3V, 32 kHz
  - < 1 µA typical standby current
