24AA00/24LC00/24C00

128-Bit I2C™ Bus Serial EEPROM

Features:

• Ìèêðîìîùíàÿ CMOS òåõíîëîãèÿ:
  -500 µA typical active current
  -250 nA typical standby current
• Organized as 16 bytes x 8 bits
• 2-wire serial interface bus, I2C™ compatible
• 100 kHz (1.8V) and 400 kHz (5V) compatibility
• Self-timed write cycle (including auto-erase)
• 4 ms maximum byte write cycle time
• 1,000,000 erase/write cycles
• ESD protection > 4 kV
• Data retention > 200 years
• 8L PDIP, SOIC, TSSOP, DFN and 5L SOT-23 packages
• Pb-free finish available
• Temperature ranges available:
  -Commercial (C):0°Cto+70°C
  -Industrial (I): -40°Cto+85°C
  -Automotive (E): -40°Cto+125°C


Description:

The Microchip Technology Inc. 24AA00/24LC00/
24C00 (24XX00*) is a 128-bit Electrically Erasable
PROM memory organized as 16 x 8 with a 2-wire
serial interface. Low-voltage design permits operation
down to 1.8 volts for the 24AA00 version, and every
version maintains a maximum standby current of only
1 µA and typical active current of only 500 µA. This
device was designed for where a small amount of
EEPROM is needed for the storage of calibration
values, ID numbers or manufacturing information, etc.
The 24XX00 is available in 8-pin PDIP, 8-pin SOIC
(150 mil), 8-pin TSSOP, 8-pin 2x3 DFN and the 5-pin
SOT-23 packages.