Support CHIPS (EPROM,EEPROM,FLASH,I2C,PIC,MCS-51,AVR, 93Cxx, ISP)

EPROM

27C64, 27C128, 27C256, 27C512, 27C010, 27C020, 27C040,27C1001
M27C1001, M27C2001, M27C4001
27C080 (A19) ,M27C801,M87C257
2716(Vpp25V),2732, (adapter DIP24)
2764, 27128, 27256, 27512, 27010,
Vpp12.5V (21Vpp Modify Circuit)

EEPROM | 28C65,28C64, 28C128, 28C256,28C512, 28C010, 28C020, 28C040 M28C16A/17A (DIP28) (Adapter or Jumper) 28C16,XLS2816 (DIP24)
FLASH Memory | 28F64, 28F128, 28F256, 28F512,28F010, 28F020 MX26C1000, MX26C2000, MX28F1000, MX28F2000 Am28F256A, Am28F512A, Am28F010A, Am28F020A (New command erase/prog.) -- intel --- i28F001BX, 28F004, 28F008, 28F016
FLASH Memory | 29F64, 29F128, 29F256, 29F512,29F010, 29F020, 29F040, 29F080 29F001,29F002, 29F004, 29F008, 29F016, 29F032
Serial (I2C) EEPROM 24Cxx | 24C02,24C04,24C08,24C16, 85C72, 85C82, 85C92 --- page write ---- 24C32,24C64,24C128,24C256,24C512

Microwire EEPROM

<------ Data 8bit -----> (pin 6 ->ORG. [Schematic connect to GND])
93C06, 93C46, 93LC46, 93C56, 93C57,
93C66, 93C76, 93C86 (8bit), AT59C11, AT59C22, AT59C13
CAT35C102, CAT35C104, CAT35C108 (pullup pin7)
<------Data 16bit------> (pin 6 ->NC [No Connect])
93C06A ,93C46X,93C56,93C66,93C76,93C86 (NS)

MicroChip PIC

16C84, 16F84, 16F84A ,16F627/16F628
12C508/A, 12C509/A, 12CE518, 12CE519, 16C505
16C620 16C621, 16C622, 16CE623, 16CE624, 16CE625, 16C710/711
---ICSP connector----
16F870, 16F871, 16F872, 16F873, 16F874, 16F876, 16F877
PIC16F873A, PIC16F874A, PIC16F876A, PIC16F877A

Atmel Flash Memory
(Sector Programming)
(Software Data Protection)

AT29C256, AT29C512,AT29C010A, AT29C020, AT29C040,AT29C040A
W29EE512,W29EE011, W29EE012, W29C020(128),W29C040
PH29EE010(W29EE011)

ASD AE29F1008 (AT29C010), AE29F2008 (AT29C020)
Ver 0.992 up(DOS). Can run under win9x
(disable prog. CPUIdle or CPUCool)

Atmel Flash Memory
AT49Fxxx (Subset 29Fxxx)
(Byte-by-Byte Programming)
(Software Data Protection)

Command seq. 5555/AA, 2AAA/55, 5555/A0
AT49F512, AT49F010, AT49F020, AT49F040
SST39SF010, SST3S9F020 ,SST39SF040
AT49F001,AT49F002 , AT49F008A
Command seq. 555/AA, 2AA/55, 555/A0
Am29F512, Am29F010, Am29F020, Am29F040,HY29F080
29F002, 29F002T, Pm29F002T

Serial Peripheral Interface (SPI)
EEPROM Mode0 (0,0)
AT25xxx, W95xxx

[Atmel] AT25010,020, 040 (A8-A0)
AT25080, 160, 320, 640, 128, 256 (A15-A0)
[ST] W95010....256, Microchip 25x010 - 25x640

--- Byte programming
25010,25020,25040
--- Page programming
25C080,25C160,25C320,25C640,25C128,25C256,25C512
AT25HP256,AT25HP512
AT25HP1024 (24bit address)

-- CAT64LCxxx (16bit DATA IN/OUT) use Socket 93Cxxx
CAT64LC010, CAT64LC020, CAT64LC040

Atmel EEPROM (page prog.) (Software Data Protection) | AT28C256, AT28C010, AT28C040
Nonvaltile SRAM (DS12xx) | DS1220,DS1225Y, DS1230Y/AB, DS1245Y/AB, DS1249Y/AB
static RAM (Test RAM) | 6116, 6264, 62256, 62512, 628128
EPROM winbond,SST Electrical Erase Chip | W27E512, W27E010, W27C010, W27C020, W27C040 SST27SF256, SST27SF512, SST27SF010, SST27SF020 MX26C4000 Vcc = 3.3-3.6V SST37VF512, SST37VF010, SST37VF020, SST37VF040
Flash Memory SST,Sanyo | SST28SF040A ,LE28F4001
| Adapter

Atmel AT89Cxx (MCS-51)
Adapter 32pin to MCS-51

Atmel Auto Setect
AT89C51,52,55, AT89LV51,52,55
AT89S8252 (8K+2K), AT89S53, AT89LS8252,AT89LS53
AT89C1051,AT89C2051,AT89C4051 (20pin)
AT89C51RC (32KB), AT89C55WD (6.2V)
SST89C54/58, SI89C52
Intel Auto Select
i87C51, i87C51FA, i87C51FB
------------------------------------------------
i8xC51,i8xC52,i8xC54,i8xC58 (tWP = 100uS*25 Pulse)

Atmel AVR 8-bit RISC AT90Sxxx (Parallel programming) Adapter 32pin to MCS-51 | (read,write,erase,verify,checkempty,Lockbits ,Fusebits) [Flash memory/EEPROM] AT90S1200,AT90S2313 90S2333, 90S4433, 90S4414, 90S8515, 90S4434, 90S8535 reference AT90S2313 pin Function Lockbit read AT90S2313 Errata Sheet.pdf

MCS-48,MCS-41
Adapter 32pin to MCS-48/41

ROM (read/verify)
P8048AH, P8049AH,P8050AH, P8042AH Vea = 12V
P8041, P8042

OTP (read/verify/Progam)
P8748,P8749H,P8742H Vea = 18V

EPROM (read/verify/Progam)
D8748,D8749,D8742,D8741, D8742 Vea = 18V

FLASH memory 8/16bit (Software Data Protection) Adapter (TSOP48) | Am29F400,Am29F800,29F160,29F320 (read,write byte mode) HY29F200, HY29F400, HY29F800 , AT49F2048A, AT49F4096A, AT49F8192A
FLASH memory 8/16bit (Vpp12V) (Software Data Protection) Adapter (TSOP48) | i28F200,i28F400,i28F800,i28F160 (TSOP48) 28F001(DIP32 or PLCC32)
EPROM 16bit (DIP40) (1-4Mbit) Adapter Eprom 16bit Eprom only | 27C1024 (27C210), 27C2048 (27C2002), 27C4096 (27C4002), Schematic by Toomas Toots (read,Program byte mode by use Resister pull up Data Bus (0xFF), A0 select low or high byte)
EPROM 16bit (DIP42) (4-32Mbit) Adapter Eprom DIP42 Eprom only | M27C400(DIP40), 27C800, 27C160, 27C322 Schematic by Toomas Toots (read,Program byte mode by use Resister pull up Data Bus (0xFF), A0 select low or high byte)
FLASH memory 8/16bit (Software Data Protection) Adapter (TSOP48LV) | 29LV200, 29LV400,29LV800,29LV160,29LV320 (read,write byte mode)

Firmware Hub / LPC FLASH
Adapter Firmware Hub/LPC (PLCC32) (PP mode) (3.3V)

-- Firmware Hub
82802AB, 82802AC, AT49LW040, AT49LW080
SST49LF002A, SST49LF003A, SST49LF004A, SST49LF008A
W49V002FA, W39V040FA

-- LPC flash
SST49LF020, SST49LF040
W49V002A, W39V040A

P28F002BC Adapter P28F002BC (DIP40) | BOOT BLOCK FLASH MEMORY - P28F002BC

28C,29F256 Shift A14 to A15 by Software
AT29C256 modify circuit pin 1( WE)