
OTP 8-Bit CMOS MCU with EEPROM Data Memory

• PIC16CE623
• PIC16CE624
• PIC16CE625

High Performance RISC CPU:

• Only 35 instructions to learn
• All single-cycle instructions (200 ns), except for
  program branches which are two-cycle
• Operating speed:
  - DC - 20 MHz clock input
  - DC - 200 ns instruction cycle
• Interrupt capability
• 16 special function hardware registers
• 8-level deep hardware stack
• Direct, Indirect and Relative addressing modes
• Interrupt capability
• 16 special function hardware registers
• 8-level deep hardware stack
• Direct, Indirect and Relative addressing modes

Peripheral Features:

• 13 I/O pins with individual direction control
• High current sink/source for direct LED drive
• Analog comparator module with:
  - Two analog comparators
  - Programmable on-chip voltage reference
  (VREF) module
  - Programmable input multiplexing from device
    inputs and internal voltage reference
  - Comparator outputs can be output signals
• Timer0: 8-bit timer/counter with 8-bit
  programmable prescaler
  
Special Microcontroller Features:

• In-Circuit Serial Programming (ICSP™) (via two
  pins)
• Power-on Reset (POR)
• Power-up Timer (PWRT) and Oscillator Start-up
  Timer (OST)
• Brown-out Reset
• Watchdog Timer (WDT) with its own on-chip RC
  oscillator for reliable operation
• 1,000,000 erase/write cycle EEPROM data
  memory
• EEPROM data retention > 40 years
• Programmable code protection
• Power saving SLEEP mode
• Selectable oscillator options
• Four user programmable ID locations
  CMOS Technology:
• Low-power, high-speed CMOS EPROM/EEPROM
  technology
• Fully static design
• Wide operating voltage range
  - 2.5V to 5.5V
• Commercial, industrial and extended temperature
  range
• Low power consumption
  - < 2.0 mA @ 5.0V, 4.0 MHz
  - 15 mA typical @ 3.0V, 32 kHz
  - < 1.0 mA typical standby current @ 3.0V
