
• PIC16C61   • PIC16C64A
• PIC16C62   • PIC16CR64
• PIC16C62A  • PIC16C65
• PIC16CR62  • PIC16C65A
• PIC16C63   • PIC16CR65
• PIC16CR63  • PIC16C66
• PIC16C64   • PIC16C67

PIC16C6X Microcontroller Core Features:

• High performance RISC CPU
• Only 35 single word instructions to learn
• All single cycle instructions except for program
  branches which are two-cycle
• Operating speed: DC - 20 MHz clock input
  DC - 200 ns instruction cycle
• Interrupt capability
• Eight level deep hardware stack
• Direct, indirect, and relative addressing modes
• Power-on Reset (POR)
• Power-up Timer (PWRT) and
  Oscillator Start-up Timer (OST)
• Watchdog Timer (WDT) with its own on-chip RC
  oscillator for reliable operation
• Programmable code-protection
• Power saving SLEEP mode
• Selectable oscillator options
  Low-power, high-speed CMOS EPROM/ROM
  technology
  Fully static design
  Wide operating voltage range: 2.5V to 6.0V
  Commercial, Industrial, and Extended
  temperature ranges
  Low-power consumption:
      ·< 2 mA @ 5V, 4 MHz
      ·15mA typical @ 3V, 32 kHz
      ·< 1mA typical standby current

PIC16C6X Peripheral Features:

• Timer0: 8-bit timer/counter with 8-bit prescaler
• Timer1: 16-bit timer/counter with prescaler,
  can be incremented during sleep via
  external crystal/clock
• Timer2: 8-bit timer/counter with 8-bit period
  register, prescaler and postscaler
• Capture/Compare/PWM (CCP) module(s)
• Capture is 16-bit, max resolution is 12.5 ns,
  Compare is 16-bit, max resolution is 200 ns,
  PWM max resolution is 10-bit.
• Synchronous Serial Port (SSP) with SPI and I2C
• Universal Synchronous Asynchronous Receiver
  Transmitter (USART/SCI)
• Parallel Slave Port (PSP) 8-bits wide, with
  external RD, WR and CS controls
• Brown-out detection circuitry for
  Brown-out Reset (BOR)


