AT90S2313

8-bit Microcontroller
with 2K Bytes of In-System Programmable Flash

Features:

• Utilizes the AVR® RISC Architecture
• AVR – High-performance and Low-power RISC Architecture
  – 118 Powerful Instructions – Most Single Clock Cycle
    Execution
  – 32 x 8 General Purpose Working Registers
  – Up to 10 MIPS Throughput at 10 MHz
• Data and Non-volatile Program Memory
  – 2K Bytes of In-System Programmable Flash
    Endurance 1,000 Write/Erase Cycles
  – 128 Bytes of SRAM
  – 128 Bytes of In-System Programmable EEPROM
    Endurance: 100,000 Write/Erase Cycles
  – Programming Lock for Flash Program and EEPROM Data
    Security
• Peripheral Features
  – One 8-bit Timer/Counter with Separate Prescaler
  – One 16-bit Timer/Counter with Separate Prescaler,
    Compare, Capture Modes and 8-, 9-, or 10-bit PWM
  – On-chip Analog Comparator
  – Programmable Watchdog Timer with On-chip Oscillator
  – SPI Serial Interface for In-System Programming
  – FullDuplexUART
• • Special Microcontroller Features
  – Low-power Idle and Power-down Modes
  – External and Internal Interrupt Sources
• • Specifications
  – Low-power, High-speed CMOS Process Technology
  – Fully Static Operation
• Power Consumption at 4 MHz, 3V, 25°C
  – Active: 2.8 mA
  – Idle Mode: 0.8 mA
  – Power-down Mode: <1 µA
• I/O and Packages
  – 15 Programmable I/O Lines
  – 20-pin PDIP and SOIC
• Operating Voltages
  – 2.7 - 6.0V (AT90S2313-4)
  – 4.0 - 6.0V (AT90S2313-10)
• Speed Grades
– 0 - 4 MHz (AT90S2313-4)
– 0 - 10 MHz (AT90S2313-10)