

• Two Wire I2C Serial Interface
   Supports 400 kHz Protocol
• Single Supply Voltage:
  – 4.5V to 5.5V for M24Cxx
  – 2.5V to 5.5V for M24Cxx-W
  – 1.8V to 3.6V for M24Cxx-R
• Hardware Write Control
• BYTE and PAGE WRITE (up to 16 Bytes)
• RANDOM and SEQUENTIAL READ
• Self-Timed Programming Cycle
• Automatic Address Incrementing
• Enhanced ESD/Latch-Up Behavior
• 1 Million Erase/Write Cycles (minimum)
• 40 Year Data Retention (minimum)