
8-Bit CMOS Microcontrollers with
A/D Converter and Capture/Compare/PWM

• PIC16C712 • PIC16C716

Microcontroller Core Features:

• High-performance RISC CPU
• Only 35 single-word instructions to learn
• All single-cycle instructions except for program
  branches which are two cycle
• Operating speed: DC – 20 MHz clock input 
  DC – 200 ns instruction cycle
• Interrupt capability
  (up to 7 internal/external interrupt sources)
• Eight-level deep hardware stack
• Direct, Indirect and Relative Addressing modes
• Power-on Reset (POR)
• Power-up Timer (PWRT) and
  Oscillator Start-up Timer (OST)
• Watchdog Timer (WDT) with its own on-chip RC
  oscillator for reliable operation
• Brown-out detection circuitry for
  Brown-out Reset (BOR)
• Programmable code-protection
• Power-saving Sleep mode
• Selectable oscillator options
• Low-power, high-speed CMOS EPROM
  technology
• Fully static design
• In-Circuit Serial Programming™ (ICSP™)
• Wide operating voltage range: 2.5V to 5.5V
• High Sink/Source Current 25/25 mA
• Commercial, Industrial and Extended temperature
  ranges
• Low-power consumption:
  - < 2 mA @ 5V, 4 MHz
  - 22.5 µA, typical @ 3V, 32 kHz
  - < 1 µA, typical standby current

Peripheral Features:

• Timer0: 8-bit timer/counter with 8-bit prescaler
• Timer1: 16-bit timer/counter with prescaler
  can be incremented during Sleep via external
  crystal/clock
• Timer2: 8-bit timer/counter with 8-bit period
  register, prescaler and postscaler
• Capture, Compare, PWM module
• Capture is 16-bit, max. resolution is 12.5 ns,
  Compare is 16-bit, max. resolution is 200 ns, 
  PWM maximum resolution is 10-bit
• 8-bit multi-channel Analog-to-Digital converter
